**Materials and Procedure:**

Erosion Lab

* Wind Erosion lab box
* Blow dryer (low then the high setting)
* Fine sand
* Regular sand
* Ruler x 2

Compression Lab

* 1000 mL beaker
* 250 mL beaker
* 200 mL of dirt
* Weigh the dirt when it is dry (200 mL)
* Pour dirt into 1000 mL beaker
* Add water (pay attention to how much you add) until the soil has absorbed its maximum
* Weigh every step to be able to make comparisons
* Dry the dirt with a paper towel and weigh it again

**Lab Report:**

Must include the following

* Hypothesis
* Procedure
* Data
* Sources of Error
* Conclusion
* Questions that you would like to research based on what you learned in this lab

Lab report due on Friday, November 2, 2018.